CTRON-MIB-NAMES DEFINITIONS ::= BEGIN

IMPORTS
    cabletron
            FROM CTRON-OIDS;

mibs OBJECT IDENTIFIER ::= { cabletron 4 }

-- MODULE-IDENTITY
--  Organization
--    Enterasys Networks
--  ContactInfo
--   "Postal:  Enterasys Networks
--             50 Minuteman Rd.
--             Andover, MA 01810-1008
--             USA
--    Phone:   +1 978 684 1000
--    E-mail:  support@enterasys.com
--    WWW:     http://www.enterasys.com"
--  Description
--    ctron-mib-names.txt
--    Revision:
--    Part Number: 
--    Date:  July 23, 2008
--    
--    REVISION     "200807231507Z"  - Wed Jul 23 15:07 UTC 2008
--    DESCRIPTION  "Added the following OIDs:
--                  ctArpAclExpMib, ctDhcpSnoopingExpMib, 
--                  ctDynamicArpInspectionExpMib."
--   
--    REVISION     "200603061501Z"  - Mon Mar  6 15:01 UTC 2006
--    DESCRIPTION  "Added the ctFastPathProtectedPortMib OID."
--   
--    REVISION     "200601161932Z"  - Mon Jan 16 19:32 UTC 2006
--    DESCRIPTION  "Added the ctDhcpServerExpMib OID."
--
--    REVISION     "200503251526Z"  - Fri Mar 25 15:26 GMT 2005
--    DESCRIPTION  "Added the ctEntityStateTC and ctEntityStateMib OIDs."
--   
--    REVISION     "200503051336Z"  - Sat Mar  5 13:36 GMT 2005
--    DESCRIPTION  "Added the ctronTrapeze OID."
--    
--    REVISION     "200410281452Z"  - Thu Oct 28 14:52 GMT 2004
--    DESCRIPTION  "Added the ctronWslMIB OID."
--    
--    REVISION     "200403251446Z"  - Thu Mar 25 14:46 GMT 2004
--    DESCRIPTION  "Added the ctronAP3000 OID."
--    
--    REVISION     "200312122049Z"  - Fri Dec 12 20:49 GMT 2003
--    DESCRIPTION  "Added the ctronV2H and v2h124-24MIB OIDs."
--    
--    This module provides authoritative definitions for part
--    of the naming tree below:
--    
--    cabletron { enterprises 52 }
--    
--    This module will be extended, as additional sub-sections
--    of this naming tree are defined.
--    
--    Enterasys Networks reserves the right to make changes in 
--    specification and other information contained in this document 
--    without prior notice.  The reader should consult Enterasys Networks
--    to determine whether any such changes have been made.
--    
--    In no event shall Enterasys Networks be liable for any incidental, 
--    indirect, special, or consequential damages whatsoever (including 
--    but not limited to lost profits) arising out of or related to this
--    document or the information contained in it, even if Enterasys
--    Networks has been advised of, known, or should have known, the 
--    possibility of such damages.
--     
--    Enterasys grants vendors, end-users, and other interested parties
--    a non-exclusive license to use this Specification in connection
--    with the management of Enterasys or Cabletron products.
--    
--    Copyright February 1999 Cabletron Systems
--    Copyright March (2000-2006) Enterasys Networks
--    
--    The assigned enterprise MIB tree for Cabletron System

ctron OBJECT IDENTIFIER ::= { mibs 1 }
-- OBJECT-IDENTITY
--  Status
--    mandatory

ctPhysical OBJECT IDENTIFIER ::= { ctron 1 }
-- OBJECT-IDENTITY
--  Status
--    mandatory

repeaterRev4 OBJECT IDENTIFIER ::= { ctPhysical 1 }
-- OBJECT-IDENTITY
--  Status
--    mandatory

chassis OBJECT IDENTIFIER ::= { ctPhysical 2 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr
--    The MMAC chassis MIB MIB.

ctPhysRptrMim OBJECT IDENTIFIER ::= { ctPhysical 3 }
-- OBJECT-IDENTITY
--  Status
--    mandatory

ctPhysModule OBJECT IDENTIFIER ::= { ctPhysical 4 }
-- OBJECT-IDENTITY
--  Status
--    mandatory

ctPModuleETWMIM OBJECT IDENTIFIER ::= { ctPhysModule 1 }
-- OBJECT-IDENTITY
--  Status
--    mandatory

ctDevice OBJECT IDENTIFIER ::= { ctPhysical 5 }
-- OBJECT-IDENTITY
--  Status
--    mandatory

ctDot5PhysMgmt OBJECT IDENTIFIER ::= { ctPhysical 6 }
-- OBJECT-IDENTITY
--  Status
--    mandatory

ctps OBJECT IDENTIFIER ::= { ctPhysical 7 }
-- OBJECT-IDENTITY
--  Status
--    mandatory

ctenv OBJECT IDENTIFIER ::= { ctPhysical 8 }
-- OBJECT-IDENTITY
--  Status
--    mandatory

ctChassis2 OBJECT IDENTIFIER ::= { ctPhysical 9 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr
--    Used for the second revision of the chassis MIB as
--    used in MMAC+ based devices.

ctUPS OBJECT IDENTIFIER ::= { ctPhysical 10 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr
--    Used for Cabletron's uninteruptable power supply MIB.

ctTRStnAssign OBJECT IDENTIFIER ::= { ctPhysical 11 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr
--    The Token Ring Station Assignment MIB.

ctResource OBJECT IDENTIFIER ::= { ctPhysical 12 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr
--    The system resource MIB which reports what's installed
--    and what's available for use.

ctIFRemap OBJECT IDENTIFIER ::= { ctPhysical 13 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr
--    MIB Allows mapping of an interface onto other interfaces.

ctIFRemap2 OBJECT IDENTIFIER ::= { ctPhysical 14 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr
--    MIB Allows mapping of an interface onto other interfaces.
--    This MIB will replace the inital ctIFRemap in future 
--    releases.

ctOrpHSIM OBJECT IDENTIFIER ::= { ctPhysical 15 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr
--     MIB used by the host platform to perform management of Orp type 
--     HSIMs.

ctPortMap  OBJECT IDENTIFIER ::= { ctPhysical 16 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr
--     This mib provides information about a  repeated ports  
--     operational mode and capability. 

ctHSIMPhysMib  OBJECT IDENTIFIER ::= { ctPhysical 17 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr
--     This mib provides information about the physical
--     operation of an HSIM.

ctCMM  OBJECT IDENTIFIER ::= { ctPhysical 18 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr
--     This branch provides information about the physical
--     operation of CMM which is a Cabletron Modem Module
--     on the AuSable product line (might branch out).


ctDataLink OBJECT IDENTIFIER ::= { ctron 2 }
-- OBJECT-IDENTITY
--  Status
--    mandatory

dot5 OBJECT IDENTIFIER ::= { ctDataLink 1 }
-- OBJECT-IDENTITY
--  Status
--    mandatory

ctsmtmib OBJECT IDENTIFIER ::= { ctDataLink 2 }
-- OBJECT-IDENTITY
--  Status
--    mandatory

ctBridge OBJECT IDENTIFIER ::= { ctDataLink 3 }
-- OBJECT-IDENTITY
--  Status
--    mandatory

ctEthernet OBJECT IDENTIFIER ::= { ctDataLink 4 }
-- OBJECT-IDENTITY
--  Status
--    mandatory

ctCSMACD OBJECT IDENTIFIER ::= { ctEthernet 1 }
-- OBJECT-IDENTITY
--  Status
--    mandatory

ctEthernetCtlParameters OBJECT IDENTIFIER ::= { ctEthernet 2 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr
--   The ctEthernetCtlParameters MIB is used to manage
--   Cabletron interfaces that comply to IEEE Draft
--   P802.3z/D4.1, IEEE Std 802.3x-1997 and IEEE Std
--   802.3y-1997.  This MIB supercedes the ctFastEthernet MIB.
 
ctFDDI OBJECT IDENTIFIER ::= { ctDataLink 5 }
-- OBJECT-IDENTITY
--  Status
--    mandatory

ctFDDIFnb OBJECT IDENTIFIER ::= { ctFDDI 1 }
-- OBJECT-IDENTITY
--  Status
--    mandatory

ctFDDIStats OBJECT IDENTIFIER ::= { ctFDDI 2 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr
--    This branch is used for all FDDI statisics values.

ctTokenRing OBJECT IDENTIFIER ::= { ctDataLink 6 }
-- OBJECT-IDENTITY
--  Status
--    mandatory

ctTokenRingFnb OBJECT IDENTIFIER ::= { ctTokenRing 1 }
-- OBJECT-IDENTITY
--  Status
--    mandatory

ctronWan OBJECT IDENTIFIER ::= { ctDataLink 7 }
-- OBJECT-IDENTITY
--  Status
--    mandatory

ctWan OBJECT IDENTIFIER ::= { ctronWan 1 }
-- OBJECT-IDENTITY
--  Status
--    mandatory

ctRemoteAccess OBJECT IDENTIFIER ::= { ctronWan 2 }
-- OBJECT-IDENTITY
--  Status
--    mandatory

ctWanServices OBJECT IDENTIFIER ::= { ctronWan 3 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr
--    Cabletron WAN Applications

ctDLSW OBJECT IDENTIFIER ::= { ctDataLink 8 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr
--    The Cabletron data link switching MIB.

ctFastEthernet OBJECT IDENTIFIER ::= { ctDataLink 9 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr
--    The cabletron fast ethernet 100Base T MIB.

ctATM OBJECT IDENTIFIER ::= { ctDataLink 10 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr
--    A branch for all Cabletron ATM MIBs.

ctATMConfig OBJECT IDENTIFIER ::= { ctATM 1 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr
--    ATM port redundancy and PVC/SVC config.

ctSwitch OBJECT IDENTIFIER ::= { ctDataLink 11 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr
--    A branch for all Cabletron Switch MIBs

ctsfSwitch OBJECT IDENTIFIER ::= { ctSwitch 1 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr
--    A branch for all Cabletron Secure Fast Switch MIBs

ctSFCS OBJECT IDENTIFIER ::= { ctsfSwitch 1 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr
--    Cabletron's Secure Fast Cell Switching MIB

ctFPS OBJECT IDENTIFIER ::= { ctSwitch 2 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr
--    The FPS configuration information and statistics MIB 

ctINB OBJECT IDENTIFIER ::= { ctDataLink 12 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr
--    A branch for all Cabletron INB MIBs

ctINBinfo OBJECT IDENTIFIER ::= { ctINB 1 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr
--    The INB configuration information and statistics MIB 

ctINBinfo2 OBJECT IDENTIFIER ::= { ctINB 2 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr
--    The INB MIB for SSX

ctBroadcast OBJECT IDENTIFIER ::= { ctDataLink 13 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr
--    The Broadcast information and configuration MIB.

ctPriorityExt OBJECT IDENTIFIER ::= { ctDataLink 14 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr
--    The ctPriorityExt Mib used to control priority packet
--    forwarding.

ctFPSServices OBJECT IDENTIFIER ::= { ctDataLink 15 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr
--    FPS Services mib
 
ctVlanExt OBJECT IDENTIFIER ::= { ctDataLink 16 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr
--    ctVlanExt MIB

ctronVVD OBJECT IDENTIFIER ::= { ctDataLink 18 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr
--    The Cabletron Voice Video and Data MIB

ctVVD OBJECT IDENTIFIER ::= { ctronVVD 1 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr
--    Voice Video and Data branch

ctVoiceOverIP OBJECT IDENTIFIER ::= { ctVVD 1 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr
--    Voice over IP mibs
  
ctCDP OBJECT IDENTIFIER ::= { ctDataLink 19 }
--OBJECT-IDENTITY
--  Status
--    optional
--  Descr

ctSmartTrunkBranch OBJECT IDENTIFIER ::= { ctDataLink 20 }
--OBJECT-IDENTITY
--  Status
--    optional
--  Descr

ctronVpnMonMIB OBJECT IDENTIFIER ::= { ctDataLink 21 }
--OBJECT-IDENTITY
--  Status
--    optional
--  Descr

ctNetwork OBJECT IDENTIFIER ::= { ctron 3 }
-- OBJECT-IDENTITY
--  Status
--    mandatory

nwDiagnostics OBJECT IDENTIFIER ::= { ctNetwork 1 }
-- OBJECT-IDENTITY
--  Status
--    mandatory


ctTranslation OBJECT IDENTIFIER ::= { ctNetwork 4 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr
--    A MIB to provide control over IP fragmentation 
--    between the various media types.

ctIGMPBranch OBJECT IDENTIFIER ::= { ctNetwork 5 }
-- OBJECT-IDENTITY
--  Status
--    mandatory

ctDirectory OBJECT IDENTIFIER ::= { ctNetwork 6 }
-- OBJECT-IDENTITY
--  Status
--    mandatory

ctAliasMib OBJECT IDENTIFIER ::= { ctNetwork 7 }
-- OBJECT-IDENTITY
--  Status
--    optional

ctApplication OBJECT IDENTIFIER ::= { ctron 4 }
-- OBJECT-IDENTITY
--  Status
--    mandatory

ctNetManagement OBJECT IDENTIFIER ::= { ctApplication 2 }
-- OBJECT-IDENTITY
--  Status
--    mandatory

ctCATV OBJECT IDENTIFIER ::= { ctApplication 3 }
-- OBJECT-IDENTITY
--  Status
--    mandatory

ctCM OBJECT IDENTIFIER ::= { ctCATV 1 }
-- OBJECT-IDENTITY
--  Status
--    mandatory

ctHETS OBJECT IDENTIFIER ::= { ctCATV 2 }
-- OBJECT-IDENTITY
--  Status
--    mandatory

ctWebView OBJECT IDENTIFIER ::= { ctApplication 4 }
-- OBJECT-IDENTITY
--  Status
--    mandatory

ctSystem OBJECT IDENTIFIER ::= { ctron 5 }
-- OBJECT-IDENTITY
--  Status
--    mandatory

ctPoMIB OBJECT IDENTIFIER ::= { ctSystem 1 }
-- OBJECT-IDENTITY
--  Status
--    mandatory

ctErrLog OBJECT IDENTIFIER ::= { ctSystem 2 }
-- OBJECT-IDENTITY
--  Status
--    mandatory

ctBackplaneProto OBJECT IDENTIFIER ::= { ctSystem 3 }
-- OBJECT-IDENTITY
--  Status
--    mandatory

ctUPowerSupply OBJECT IDENTIFIER ::= { ctSystem 4 }
-- OBJECT-IDENTITY
--  Status
--    mandatory

ctFpRedundancy OBJECT IDENTIFIER ::= { ctSystem 5 }
-- OBJECT-IDENTITY
--  Status
--    mandatory

ctTrapTable OBJECT IDENTIFIER ::= { ctSystem 7 }
-- OBJECT-IDENTITY
--  Status
--    mandatory

ctDownLoad OBJECT IDENTIFIER ::= { ctSystem 8 }
-- OBJECT-IDENTITY
--  Status
--    mandatory

ctPIC OBJECT IDENTIFIER ::= { ctSystem 9 }
-- OBJECT-IDENTITY
--  Status
--    mandatory

ctFlash OBJECT IDENTIFIER ::= { ctSystem 10 }
-- OBJECT-IDENTITY
--  Status
--    mandatory

ctLFAP OBJECT IDENTIFIER ::= { ctSystem 11 }
-- OBJECT-IDENTITY
--  Status
--    mandatory

ctTxQArb OBJECT IDENTIFIER ::= { ctSystem 12 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr
--    This MIB provides configuration for the priority in
--    which transmit queues are serviced for Cabletron
--    devices that support multiple transmit queues.

ctDcm OBJECT IDENTIFIER ::= { ctron 6 }
-- OBJECT-IDENTITY
--  Status
--    mandatory

ctTrapLog OBJECT IDENTIFIER ::= { ctron 44 }
-- OBJECT-IDENTITY
--  Status
--    mandatory

ctronExp OBJECT IDENTIFIER ::= { mibs 2 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr
--    This branch is for all non-accepted Cabletron
--    Proprietary MIBs.

ctronDLM OBJECT IDENTIFIER ::= { ctronExp 1 }
-- OBJECT-IDENTITY
--  Status
--    mandatory

-- ctronSFPS OBJECT IDENTIFIER ::= { ctronExp 3 }
-- OBJECT-IDENTITY
--  Status
--    deprecated
--  Descr
--    This MIB has been moved to ctSFPS { ctDataLink 17 }


-- ctronSwitch OBJECT IDENTIFIER ::= { ctronExp 4 }
-- OBJECT-IDENTITY
--  Status
--    deprecated
--  Descr
--    This MIB branch has been approved and moved to ctSwitch
--    { ctDataLink 11 }

ctLicense OBJECT IDENTIFIER ::= { ctronExp 5 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr
--    The experimental application download license MIB.

ctX25 OBJECT IDENTIFIER ::= { ctronExp 6 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr
--    The experimental branch for WAN X.25 MIB.

ctFault OBJECT IDENTIFIER ::= { ctronExp 7 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr
--    The experimental branch for the fault MIB.

ctGateway OBJECT IDENTIFIER ::= { ctronExp 8 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr
--    The SPMA gateway agent.

ctronHost OBJECT IDENTIFIER ::= { ctronExp 9 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr
--    The SPMA host MIB.

ctronRunTimeDiag OBJECT IDENTIFIER ::= { ctronExp 10 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr
--    This is the experimental branch for run time
--    diagnostic development.

ctProfiler OBJECT IDENTIFIER ::= { ctronExp 11 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr
--    This is the experimental branch for the profiler MIB.
--    This will be used until we get a good feeling for what
--    needs to be in the profiler.

ctVLANMib OBJECT IDENTIFIER ::= { ctronExp 12 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr
--    This is the experimental MIB branch for virtual LAN.

-- ctronFlashFS OBJECT IDENTIFIER ::= { ctronExp 13 }
-- OBJECT-IDENTITY
--  Status
--    deprecated
--  Descr
--    This is used for experimental MIB for the flash file system.
--
--    This MIB has been approved as an official Cabletron MIB.

ctDistMgt OBJECT IDENTIFIER ::= { ctronExp 14 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr
--    This branch is used for experimental distributed management
--    objects.

ctRmonDebug OBJECT IDENTIFIER ::= { ctronExp 15 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr
--    RMON Debug MIB

-- ctLoadShare OBJECT IDENTIFIER ::= { ctronExp 16 }
-- OBJECT-IDENTITY
--  Status
--    deprecated
--  Descr
--    This branch is used for the experimental load sharing MIB.
--
--    This MIB has been accepted and is now a group under the ctBridge MIB.
--    {ctBridge 10}

ctNetSim OBJECT IDENTIFIER ::= { ctronExp 17 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr
--    Spectrum Network Simulation MIB

--ctFPSServices OBJECT IDENTIFIER ::= { ctronExp 18 }
-- OBJECT-IDENTITY
--  Status
--    deprecated
--  Descr
--    FPS Services mib 
--
--    This MIB has been accepted and is now off the ctDataLink 15.
 
--ctPriorityExt OBJECT IDENTIFIER ::= { ctronExp 19 }
-- OBJECT-IDENTITY
--  Status
--    deprecated
--  Descr
--    ctPriorityExt MIB
--
--    This MIB has been accepted and is now off the ctDataLink 14.

--ctVlanExt OBJECT IDENTIFIER ::= { ctronExp 20 }
-- OBJECT-IDENTITY
--  Status
--    deprecated
--  Descr
--    ctVlanExt MIB
--
--  This MIB has been accepted and is now off the ctDataLink 15.

--ctDefaults OBJECT IDENTIFIER ::= { ctronExp 21 }
-- OBJECT-IDENTITY
--  Status
--    optional
--  Descr
--    This MIB is used to clear the device.
-- This MIB has been accepted and is now off the internal directory.

ctMemory OBJECT IDENTIFIER ::= { ctronExp 22 }
-- OBJECT-IDENTITY
-- Status
--   optional
-- Descr
--   This MIB used for the implementation of memory management functionality.

ctEngTest OBJECT IDENTIFIER ::= { ctronExp 23 }
-- OBJECT-IDENTITY
--  Status
--    optional
--  Descr

flowPolicyPolling OBJECT IDENTIFIER ::= { ctronExp 24 }
-- OBJECT-IDENTITY
--  Status
--    optional
--  Descr

--catnet OBJECT IDENTIFIER ::= { ctronExp 25 }
-- OBJECT-IDENTITY
--  Status
--    deprecated
--  Descr
--     This mib has been moved to Application 3.

-- monLfap OBJECT IDENTIFIER ::= { ctronExp 26 }
-- OBJECT-IDENTITY
--  Status
--    deprecated
--  Descr
--    This mib has been moved to ctSystem 11.

ctDemandAccess OBJECT IDENTIFIER ::= { ctronExp 27 }
-- OBJECT-IDENTITY
--  Status
--    optional
--  Descr

ctHWDebug  OBJECT IDENTIFIER ::= { ctronExp 28 }
-- OBJECT-IDENTITY
--  Status
--    optional
--  Descr
--    This mib is for specific hardware debug
--    it will be filled in as needed. Currently
--   (12/98) the only item under here is isp info.

ctFWDebug  OBJECT IDENTIFIER ::= { ctronExp 29 }
-- OBJECT-IDENTITY
--  Status
--    optional
--  Descr
--    This mib is for specific firmware debug
--    it will be filled in as needed. 

ctEntityStateTC  OBJECT IDENTIFIER ::= { ctronExp 30 }
-- OBJECT-IDENTITY
--  Status
--    optional
--  Descr
--    This is an OID registration for the draft entityStateTc Module.

ctEntityStateMib  OBJECT IDENTIFIER ::= { ctronExp 31 }
-- OBJECT-IDENTITY
--  Status
--    optional
--  Descr
--    This is an OID registration for the draft entityStateMIB Module.

ctDhcpServerExpMib  OBJECT IDENTIFIER ::= { ctronExp 32 }
-- OBJECT-IDENTITY
--  Status
--    optional
--  Descr
--    This is an OID registration for a third party DHCP server MIB.

ctFastPathProtectedPortMib  OBJECT IDENTIFIER ::= { ctronExp 33 }
-- OBJECT-IDENTITY
--  Status
--    optional
--  Descr
--    This is an OID registration for a third party protected port MIB.

ctArpAclExpMib  OBJECT IDENTIFIER ::= { ctronExp 34 }
-- OBJECT-IDENTITY
--  Status
--    optional
--  Descr
--    This is an OID registration for a third party ARP ACL MIB.

ctDhcpSnoopingExpMib  OBJECT IDENTIFIER ::= { ctronExp 35 }
-- OBJECT-IDENTITY
--  Status
--    optional
--  Descr
--    This is an OID registration for a third party DHCP snooping MIB.

ctDynamicArpInspectionExpMib  OBJECT IDENTIFIER ::= { ctronExp 36 }
-- OBJECT-IDENTITY
--  Status
--    optional
--  Descr
--    This is an OID registration for a third party dynamic ARP 
--    inspection MIB.

ctronExtn OBJECT IDENTIFIER ::= { mibs 3 }
-- OBJECT-IDENTITY
--  Status
--    mandatory

ctronChassis OBJECT IDENTIFIER ::= { ctronExtn 1 }
-- OBJECT-IDENTITY
--  Status
--    mandatory

ctronRmon OBJECT IDENTIFIER ::= { ctronExtn 2 }
-- OBJECT-IDENTITY
--  Status
--    mandatory

ctronMib2 OBJECT IDENTIFIER ::= { ctronExtn 3 }
-- OBJECT-IDENTITY
--  Status
--    mandatory

ctActions OBJECT IDENTIFIER ::= { ctronExtn 4 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr
--    Definitions of the event actions MIB.  This is an
--    extension to RMON alarms and events.

ctAtmfLanEmulation OBJECT IDENTIFIER ::= { ctronExtn 5 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr
--    MIB for managing configuration data for ATM Emulated LANs.

ctLeClient OBJECT IDENTIFIER ::= { ctAtmfLanEmulation 1 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr

ctElan OBJECT IDENTIFIER ::= { ctAtmfLanEmulation 2 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr

ctLes OBJECT IDENTIFIER ::= { ctAtmfLanEmulation 3 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr

ctBus OBJECT IDENTIFIER ::= { ctAtmfLanEmulation 4 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr

ctMidManager OBJECT IDENTIFIER ::= { mibs 4 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr
--    This branch is used for all MID level manager MIBs.

ctGateWay OBJECT IDENTIFIER ::= { ctMidManager 1 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr
--    This is used for the SPMA Gateway agent.

ctronV2H OBJECT IDENTIFIER ::= { mibs 12 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr
--    This branch is used for the V2H.

v2h124-24MIB OBJECT IDENTIFIER ::= { ctronV2H 30 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr
--    This is the V2H MIB.

ctronAP3000 OBJECT IDENTIFIER ::= { mibs 13 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr
--    This branch is used for the AP3000.

ctronWslMIB OBJECT IDENTIFIER ::= { mibs 14 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr
--    This branch is used for the Wsl MIB.

ctronTrapeze OBJECT IDENTIFIER ::= { mibs 15 }
-- OBJECT-IDENTITY
--  Status
--    mandatory
--  Descr
--    This branch is used for the Trapeze MIBs.

ctronInternal OBJECT IDENTIFIER ::= { mibs 100 }
-- OBJECT IDENTITY
--  Status
--    optional
--  Descr
--    This is the internal directory.

ctDefaults OBJECT IDENTIFIER ::= { ctronInternal 1 }
-- OBJECT IDENTITY
--  Status
--    optional
--  Descr
--    This branch is for the defaults mib.

ctEnet OBJECT IDENTIFIER ::= { ctronInternal 2 }
-- OBJECT IDENTITY
--  Status
--    optional
--  Descr
--    This branch is for the Enet mib.

END
